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/A 202000 An incorzect timescale is selected for the Verilog Oucput (.VO) file of this PLL design. Io's required That the Timescale s
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管脚分配
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控制模块
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分频模块
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显示模块
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