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程序文件
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input pass_key,
output reg red_led,
output reg green_led,
output [3:0] bit_select.
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eg [31:0] data_cnt=32"d0;

freg clk_1Hz=0;

2 1wavs@ (posedze clk_100M)

i (data_cnt>=32’ d100_000_000;
data_cnt<=32"d0;

else
data_cnt{=data_cnt+32’d1;
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[ 1ways@(posedze clk_100M)

if (data_ent>=32" d50_000_000)
clk_1Hz<=0:
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程序编译
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管脚约束
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eer \ Light/red_green Light. srcs/ constrs_L/new/pins.

set_property PACKAGE_PIN W5 [get ports clk_100M]
set_property IOSTANDARD LVCMOS33 [get_ports clk_100M]
create_clock —add —name sys_clk_pin —period 10.00 —waveform {0 5} [get_ports clk_100M]

set_property PACKAGE_PIN U18 [get_ports pass_key]
set_property IOSTANDARD LVCMOS33 [get_ports pass_key]

set_property PACKAGE_PIN Ul6 [get ports red_led]
set_property IOSTANDARD LVCMOS33 [get_ports red_led]
set_property PACKAGE_PIN E19 [get ports green_led]
set_property IOSTANDARD LVCMOS33 [get_ports green_led]

)] lednum select,

output [7:
0] bit_select

output [

set_property PACKAGE_PIN W7 [get_ports lednum_select[0]]
set_property IOSTANDARD LVCMOS33 [get ports lednum_select[0]]
set_property PACKAGE_PIN W6 [get ports lednum_select[1]]
set_property IOSTANDARD LVCMOS33 [get ports lednum_select[1]]
set_property PACKAGE_PIN U8 [get_ports lednum_select[2]]
set_property IOSTANDARD LVCMO0S33 [get ports lednum select[2]]
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esictop/M021 /r = \ Light/red_green Light. srcs/ constrs_L/new/pins.

PACKAGE_PIN U8 [get_ports lednum select[2]]
TOSTANDARD LVCMOS33 [get_ports lednum_select[2]]
PACKAGE_PIN V8 [get_ports lednum _select[3]]
TOSTANDARD LVCMOS33 [get_ports lednum_select[3]]
PACKAGE_PIN U5 [get_ports lednum _select[4]]
TOSTANDARD LVCMOS33 [get_ports lednum_select[4]]
PACKAGE_PIN V5 [get_ports lednum select[5]]
TOSTANDARD LVCMOS33 [get_ports lednum_select[5]]
PACKAGE_PIN U7 [get_ports lednum _select[6]]
TOSTANDARD LVCMOS33 [get_ports lednum_select[6]]
PACKAGE_PIN V7 [get_ports lednum select[7]]
TOSTANDARD LVCMOS33 [get_ports lednum_select[7]]

PACKAGE_PIN U2 [get_ports bit_select[0]]
TOSTANDARD LVCMOS33 [get_ports bit_select[0]]
PACKAGE_PIN U4 [get_ports bit_select[1]]
TOSTANDARD LVCMOS33 [get_ports bit_select[1]]
PACKAGE_PIN V4 [get_ports bit_select[2]]
TOSTANDARD LVCMOS33 [get_ports bit_select[2]]
PACKAGE_PIN W4 [get_ports bit_select[3]]
TOSTANDARD LVCMOS33 [get_ports bit_select[3]]




