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程序文件
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程序编译
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BllType  ID  Message
( 332001 The selected device family is not supported by the report_metastability command.
332102 Design is not fully constrained for setup requirements

Quarcus IT 64-Bit TimeQuest Timing Analyzer was successful. 0 errors, 3 warnings
Running Quartus II 64-Bit EDA Netlist Writer
Command: quartus_eda —-read settings files-off --write settings files=off taxi fee -c taxi fee
204018 Generated files "taxi fee.vho" and "taxi fee vhd.sdo" in directory "F:/QUARTUS program/taxi VEDL Y081/taxi VEDL sim/simulation/modelsim/" for EDA simslatic
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管脚分配
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> 9 Node Name: Direction Location 1o Bank VREFGroup  Fitterlocaton  1/0Standard
& "l acn Tt Lz 1 BN o 331y, defaul)
2 | (I reset Tnput PN A 2 8280 PN A 331V, defoul)
24 SEG[7] Output PIN_M3 1 B1N2 PIN_M3. 3.3-VLV..default)
o4 secle] output N1 1 BN N1 3391V, defoul)
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