工程文件
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程序文件
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D PROCESS (clk_liaoyuging)
BEGIN
g TF (clk_licoyuging'EVENT 2ND clk_lisoyuging = '1') THEN
& IF (zsc_n_liaoyuqing = '0') THEN--EL
Predefined sequence liaoyuging <-| "ii0iot01" | -ERet BT, AEHAEEFRFFF (of)
= LsE
Predefined_sequence_liaoyuging <= Predefined_sequence_liaoyuging;
=D TF;
=D TF;
END PROCESS;




[image: image3.png][LIBRARY iecee;
USE ieee.std_logic_1164.all;
USE ieee.std_logic_unsigned.all;

PORT (

clk_liaoyuging : IN STD_LOGIC,
rst_n_liaoyuging : IN STD_LOGIC; -
sequence_out_liaoyuging : OUT STD LOGIC

)i
END Synchronous_sequence_liaoyuging;

SIGNAL Predefined sequence liaoyuging :
SIGNAL Sync_sequence_liaoyuging_out : STD LOGIC 07
SIGNAL count_liaoyuging : STD_LOGIC_VECTOR(2 DOWNTO 0) :

PROCESS (clk_liaoyuging)
BEGIN
IF (clk_liaoyuging'EVENT AND clk_liao
IF (rst_n_liaoyuging = '0') THEN
Predefined sequence_liaoyuging <

ELSE o S ————————
DPredefine: P

ging = '1') THEN





管脚分配
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Location 1joBank \VREF Group 1/ Standard Reserved Current Strength Slew Rate Differential Pair
PIN_23 1 B1NO 2.5V (default) 8mA (defauit)
PIN_25 2 B2_NO. 2.5V (default) 8mA (default)
PIN_28. 2 | B2.NO 2.5V (default) 8mA (default) 2 (default)




仿真测试文件

[image: image5.png][EENTITY Synchronous_sequence liaoyuqging_vhd_tst IS
REND Synchronous_sequence_liaoyuging vhd_tst:
[EARCHITECTURE Synchronous_sequence liaoyuqing_arch OF Synchronous_sequence_liaoyuging vhd_tst IS

SIGNAL clk_liaoyuging : STD_LOGIC;

SIGNAL rst_n_liaoyuging : STD LOGIC;

SIGNAL sequence_out_liaoyuging : STD LOGIC;
[EICOMPONENT Synchronous_sequence_liaoyuging
PORT (

clk_liaoyuging : IN STD_LOGIC;
rst_n_liaoyuging : IN STD_LOGIC;
sequence_out_liaoyuging : OUT STD_LOGIC
)i

END COMPONENT;

[BEGIN

il : Synchronous_sequence_liaoyuging
PORT MAP (

list t 1 m
clk_liaoyuging => clk_liaoyuging,
rst_n_liaoyuging => rst_n_liaoyuging,
sequence_out_liaoyuging => sequence_out_liaoyuging

PROCESS

rst_n_liaoyuging<
wait for 200ns;

rst_n_liaoyuging<='1';
WA T





仿真图
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