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程序文件
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Type ID Message
() 208019 Generatea file
204019 Generated file
() 208019 Generated file
204019 Generated file
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204019 Generated file
() 208019 Generated file

>

ages

top_8_1200mv_0c_slow.vo in folder "F:/QUARTUS_program/pingpang_fifo_z429/pingpang_fifo/simulation/modelsim/" for EDA simulation tool
top_min_1200mv_0c_fast.vo in folder "F:/QUARTUS program/pingpang_fifo_z429/pingpang_fifo/simulation/modelsim/" for EDA simlation tool
top.vo in folder "F:/QUARTUS program/pingpang_fifo_z429/pingpang_fifo/simulation/modelsim/" for EDA simulation tool
top_8_1200mv_85c_v_slow.sdo in folder "F:/QUARTUS program/pingpang_fifo_z429/pingpang_fifo/simulation/modelsim/" for EDA simulation tool
top_8_1200mv_0c_v_slow.sdo in folder "F:/QUARTUS_program/pingpang_fifo_Z429/pingpang fifo/simulation/modelsim/" for EDA simulation tool
top_min_1200mv_0c_v_fast.sdo in folder "F:/QUARTUS_program/pingpang_fifo_2429/pingpang_fifo/simulation/modelsim/" for EDA simulation tool
top_v.sdo in folder "F:/QUARTUS_program/pingpang_fifo_2429/pingpang_fifo/similation/modelsim/" for EDA simulation tool

Quartus II 64-Bit EDA Netlist Writer was successful. 0 errors, 0 warnings
() 293000 Quartus IT Full Compilation was successful. 0 errors, 11 warnings
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程序编译
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Type ID Message
() 204019 Generatea file top_8_1200mv_0c_slow.vo in folder "F:/QUARTUS_program/pingpang_fifo_2429/pingpang_fifo/simalation/modelsim/" for EDA simalation tool
204019 Generatea file top_min_1200mv_Oc_fast.vo in folder "F:/QUARTUS_program/pingpang_fifo_2429/pingpang_fifo/similation/modelsin/" for EDA simulation tool
204019 Generated file top.vo in folder "F:/QUARTUS_program/pingpang fifo_Z429/pingpang fifo/similation/modelsim/" for EDA simulation tool
() 204019 Generated file top & 1200mv_gSc v_slow.sdo in folder "F:/QUARTUS program/pingpang £1fo Z42/pingpang £ifo/sim:lation/modelsim/" for EDA simlation tool
204019 Generated file top_8_1200mv_0c_v_slow.sdo in folder "F:/QUARTUS_program/pingpang fifo_2429/pingpang_fifo/simulation/modelsim/" for EDA simulation tool
204019 Generated file top_min_1200mv_0c_v_fast.sdo in folder "F:/QUARTUS_program/pingpang_fifo_2429/pingpang_fifo/simulation/modelsin/" for EDA simulation tool
() 204019 Generatea file top_v.sdo in folder "F:/QUARTUS program/pingpang_fifo_7429/pingpang_fifo/simalacion/modelsim/" for EDA simalation tool
> Quartus II €4-Bit EDA Netlist Writer was successful. 0 errors, 0 warnings
gl| @ 293000 Quarcus IT Full Compilation was successful. 0 errors, 11 warnings
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Testbench
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仿真图
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