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Found 2 design units,
Elaborating entity "pwm" for the top level hierarchy
Warning: Clock miltiplexers are found and protected

Info: Implemented 62 device resources after synthesis - the final resource count might be different
Info: Quartus IT Analysis s Synthesis was successful. 0 errors, 2 warnings
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