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程序编译
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532140 No Removal paths to report
() 332140 No Minimm Pulse Width pachs to report
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332102 Design is not fully constrained for setup requirements
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Quarcus IT 64-Bit TimeQuest Timing Analyzer was successful. 0 errors, 2 warnings
) Running Quartus II 64-Bit EDA Netlist Writer
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管脚分配
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Testbench
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25 | Bep_sn=s'b0020;
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30 | #i00;
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