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程序编译
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Analysis & Synthesis was successful (4 warnings)

otal PLLs

Running Quarcus 11 Analysis & Synthesis

Elaborating entity "led_led” for the top level hierarchy

Warning (10540): VEDL Signal Declaration warning at led_led.vhd(24):
Warning (10540): VEDL Signal Declaration warning at led_led.vhd(25):
Warning (10540): VADL Signal Declaration warning at led_led.vhd (26)
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Command: quartus_map --read_settings_files=on —-write_settings_files=off led led -c led_led
Found 2 design units, including 1 entities, in source file lcd_lcd.vhd
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Info: Implemented 21 device resources after synthesis - the final resource count might be different
Info: Quartus IT Analysis s Synthesis was successful. 0 errors, 4 warnings

signal "hspw” because signal was never assigned a value
signal "hbpd” because signal was never assigned a value
signal "hozval” because signal was never assigned a value
signal "hfpd” because signal was never assigned a value





仿真文件
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仿真图
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定义的HSPW为3，所以高电平为4个时钟
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