工程文件
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程序文件

[image: image2.png]nodule meteor_led (
input clk,

input reset,
output [15:0] led
)i

reg [7:0] pwm_count=8'd0;

always@ (posedge clk)

if(reset)

pwm_count<=8'd0;

else

if (pwm_count>=8"'d16)
pwm_count<=8'd0;

else]
pwm_count<=pwm_count+8'dl;




程序运行
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RTL图
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状态图
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程序仿真
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