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204019 Generated file traffic_light_min_1200mv_Oc_fast.vo in folder "D:/A_workarea/QUARTUS program/traffic_light_key_2838/craffic_light/simulavion/modelsin/" for EDA :

204019 Generated file traffic light.vo in folder "D:/A workarea/QUARTUS program/traffic 1ight key Z838/traffic light/similation/modelsim/" for EDA simlation tool

() 204019 Generated file traffic light & 1200mv_gSc v_slow.sdo in folder "Di/A workarea/QUARTUS progzam/traffic light key 2838/craffic light/simulation/modelsim/" for ED:
204019 Generated file traffic light 8 1200mv_0c_v_slow.sdo in folder "D:/A workarea/QUARTUS program/traffic_light_key Z838/traffic_light/simulation/modelsim/" for EDA

204019 Generated file traffic_light_min_1200mv_Oc_v_fast.sdo in folder "D:/A workarea/QUARTUS program/traffic_light_key_2838/traffic_light/simulavion/modelsin/" for EI

() 204019 Generated file traffic_light_v.sdo in folder "D:/A_workarea/QUARTUS program/traffic_light_key 2838/traffic_light/simulavion/modelsin/" for EDA simulation tool

Quartus II 64-Bit EDA Netlist Writer was successful. 0 errors, 0 warnings
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25 | . main red(main_req),//E8]
24 | . main green(main_green),//ZH4]
25 | . main vellow(main yellow),//ZH#iT

27 | . branch red(oranch_req), /S8
28 | . pranch green (branch_green),//SHi]
23 | . branch yellow(branch yellow),//SH#iT

31 . weixuan(weixuan),//HBE ik
32 . duanxian(duanxian)//HBERE
33 ()

35 [Hinicial begin
36 [ lock key=
37 | #100000,
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仿真图
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分频模块
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控制模块
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倒计时模块
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显示模块
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