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程序文件
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程序编译
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Bllzype 1D Message
> @ 12021 Found 1 design units, including 1 entities, in source file db/add_sub_8pc.tdf
12130 Elaborated megafunction instantiation "displayl226:i_display|lpm divide:Div0"
12133 Instantiated megafunction "displayl226:i display|lpm divide:Div0" with the following parameter:
12021 Found 1 design units, including 1 entities, in source file db/lpm_divide_agm.tdf
(286030 Timing-Driven Synthesis is running
$ 170493 registers lost all their fanouts during netlist optimizations.
16010 Generating hard block partition "hard block:auto_generated inst"
@ 21057 Implemented 570 device resources after synthesis - the final resource count might be different
[} Quartus IT 64-Bit Analysis & Synthesis was successful. 0 errors, 0 warnings

sages
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仿真图
整体仿真
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按键上升沿模块仿真
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控制模块仿真
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显示模块仿真
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