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2 [module acclé(
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S alwayse (posedge clk, negedge rst)
10 1£(1zst)

11 o=0;

12 else

13 c=cta;

1 endmodule




Testbench
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程序编译
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(A Transcript

¢ Compile of accls.v vas successtul.
¢ Compile of accis_tb.v vas successful.
¢ 2 compiles, 0 failed with no errors.





仿真图
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改成模拟波形显示
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