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程序文件
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程序编译
[image: image3.png]4 P Compile Design

> B Anayss aSynthess & Quartus Tl
P Fitter (Place &Route)
P Assemiier (Generate rog @ FullCompiation was successfl (11 warrings)

> TmeQuest g s
(Er=|

»
»
»
b b EDANesstwiter
1 ProgramDevie (Open Prora

il 3

status.

Modue

Ful Compiation
Analysis & Synthesis

EDA Netist Writer

i | il i D

P <<sech>> v

T i ]
HElRIR N
RlType D Message

b @ Quartus IT 64-Bit EDA Netlist Writer was successful. 0 errors, 0 warnings
(293000 Quartus II Full Compilation was successful. 0 errors, 11 warnings





RTL图
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管脚分配
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Testbench
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END PROCESS init;

END Alarm_16_arch;




仿真图
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