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程序文件
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input clk, //EtEs
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4 input k1,//FF85
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input k2,//EfF. #E&-FET
input k3,//8&fL
input k4, //i&FE30F0IE AR 60%

; output [5:0] time_cnt //%iHi @A
9 )i
* 10
% 11  //parameter CNT=32'd50_000_000;// kiR Fli%6]
0 12 parameter CNT=32'd50;//{5EFHi%E)
s 13
oierarchy [ B Fis ] & Design Urits 5} 14 //4539RE|1Hz
———————n 15 reg [31:0] count;
fow mmloin =] a 16 reg clk 1Hz;
e — 17 always@(posedge clk or negedge k3)
> Comeils Do 18 =  if(!k3)begin
> 19 clk_1Hz<=0;
P Fitter (Place & Route) 20 count<=32'd0;
W Assenbler (Generate progr 21 end
W Classic Tining Analysis |
B Netlist triter 22 else if(state==sl || state==s4)
| ® Frogran Device (Open Frogram 23 = if (count>=CNT)begin/ /%L
24 count<=32'd0;
25 clk_1Hz<=1;//1%};
26 end
27 = else begin
28 count<=count+32'dl;
29 clk_1Hz<=0;
30 end
31 = else begin
32 count<=32'd0;
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程序编译
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Tnfo: Found 1 design units, including 1 entities, in source file down cnt.v

Info: Elaborating entity "down_cnt” for the top level hierarchy
Info: 4 registers lost all their fanouts during netlist oprimizations. The first 4 are displayed below.
Info: Implemented 74 device resources after synthesis - the final resource count might be different

Info: Quartus IT Analysis & Synthesis was successful. 0 errors, 0 warnings




仿真图
60秒倒计时
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60秒倒计时局部
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60秒倒计时局部
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30秒倒计时
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