数码管电路
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工程文件
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程序文件
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程序编译
[image: image5.png][Project Navigator 1Ex| @ ‘Compiation Report - segment
Entty
Ay cydone: EP1C3T100C8 Flow Status. ‘Successful - Thu Oct 21 23:18:11 2021
8 segment |Quartus T1 64t Version 13,0, 1Buid 232 06/12/2013 5P 153 Ful Version
Revison Name: segent
TopievelEntity Name  segment
Famiy Cydone
Device EpicsTIo0cs
Timing Models Fral
. Totalogic dements 0/2910(0%)
K Totalpins 21/65(32%)
Total virtual pins o
" Total memary bits 0/59,904(0%)
(23 TimeQuest Tning Anf| TotalPLLs 0/1(0%)
b (20 EDANetist Writer
) Flow Messages
< ] v || (D) Fow Suppressed e
B vierarchy Fies | pesontnts | © 4[»
frass Tax|

@ QuartusTl

o —
=

4 P Compie Design

> b ardys asmvess
> it e aae) e
P Assembler (Generate programming files)
[ T ——
> Attt
4 Program Device (Open Programmer)

@ FullComplaton was successful (29 warnings)

3
3
3
3

“ i D





管脚分配
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