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程序编译
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Found 2 design units, including 1 entities, in source file cimer.vhd
Found 1 design units, including 1 entities, in source file Time_cnt.bdf

Elaborating entity "time_cnt” for the top level hierarchy

Elaborating entity "timer” for hierarchy "timer:instl”

Elaborating entity "div" for hierarchy "diviinst”

Inplemented 25 device resources after synthesis - the final resource count might be different
Quartus 11 Analysis & Synthesis was successful. 0 errors, 0 warmings
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仿真图
整体仿真图
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计时到59后回到0
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分频模块仿真图
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计时模块仿真图
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